**Shipper’s Declaration for Section II Lithium Cells / Batteries**

**WARNING: LITHIUM BATTERIES IDENTIFIED BY THE MANUFACTURER AS BEING DEFFECTIVE FOR SAFETY REASONS, OR THAT HAVE BEEN DAMAGED, MUST NOT BE SHIPPED BY AIR.**

**Shipment Details:**

Master Air Waybill Number:

(For Direct Shipment)

House Air Waybill Number:

(If applicable)

**Shipper’s Information:**

Name: Address:

Contact Number:

Select the applicable battery type(s) and fill in the blanks:

Origin (Optional):

Destination (Optional):

**Consignee’s Information:**

Name: Address:

Contact Number:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Battery Type [IMP Code]** | | **IATA Limitation** | **Piece (No of Carton)** | **Net Weight/ Qty per Package (kg)** |
| **UN3480 | PI965 [ELI]** Lithium Ion Cells / Batteries ONLY | Cell / Battery ≤ 2.7Wh | *No. of Pieces: No Limit Max Net Battery Weight 2.5 kg per package* |  |  |
| Cell > 2.7 Wh but ≤ 20 Wh | *No. of Pieces: Max 8 Cells  per package* |  |  |
| Battery > 2.7 Wh but ≤ 100 Wh | *No. of Pieces: Max 2 Batteries  per package* |  |  |
| **UN3481 | PI966 [ELI]** Lithium Ion Cells / Batteries Packed with Equipment | | *Cell ≤ 20Wh or  Battery ≤ 100Wh  Max Net Battery Weight 5 kg per package* |  |  |
| **UN3481 | PI967 [ELI]** Lithium Ion Cells / Batteries Contained in Equipment | |  |  |
| **UN3090 | PI968 [ELM]** Lithium Metal Cells / Batteries ONLY | Cell / Battery ≤ 0.3g lithium | *No. of Pieces: No Limit  Max Net Battery Weight 2.5 kg per package* |  |  |
| Cell > 0.3g but ≤ 1g lithium | *No. of Pieces: Max 8 Cells  per package* |  |  |
| Battery > 0.3g but ≤ 2g lithium | *No. of Pieces: Max 2 Batteries  per package* |  |  |
| **UN3091 | PI969 [ELM]** Lithium Metal Cells / Batteries Packed with Equipment | | *Cell ≤ 1g lithium or  Battery ≤ 2g lithium Max Net Battery Weight 5 kg per Package* |  |  |
| **UN3091 | PI970 [ELM]** Lithium Metal Cells / Batteries Contained in Equipment | |  |  |

 Lithium  **ION** batteries in compliance with Section II of PI .

 Lithium  **METAL** batteries in compliance with Section II of PI .

 This package does not contain any damaged and / or defective cells and / or batteries.

 This package must be handled with care. A flammability hazard exists if the package is damaged.

 Special procedures must be followed in the event the package is damaged, to include inspection and repacking if necessary.

Special Procedures:  *(E.g. Follow Special Procedures as per MSDS Section xx to xx in the event the package is damaged)*

Telephone Number for Additional Information:

(Country Code) + Area Code + Phone Number

 Remarks:

**Full Name:**

(Capital Letter)